Profile leveling is generally required by the designer to determine the elevation of points over a specific route such as road mark, railway, canal or a pipe line alignment.The procedure for determining the difference in elevation between two points has already been done in previous practical.
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