Instruction Cycle• Each phase decomposed into sequence of elementary micro-operations• E.g. fetch, indirect, and interrupt cycles• Execute cycle—One sequence of micro-operations for each opcode• Need to tie sequences together• Assume new 2-bit register—Instruction cycle code (ICC) designates which part of cycle processor is in– 00: Fetch– 01: Indirect – 10: Execute – 11: Interrupt
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