On two-stroke diesels an electrically driven auxiliary blower is usually provided because are availahthe exhaust gas driven turboblower cannot provide enough air at low engine speeds, and the pressurized air is usually cooled to increase the charge air density.
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