As the gate voltage increases in the negative direction, the depletion region widens, which reduces the effective width of the channel. This leads to a decrease in the current flowing from the source to the drain (I_D).
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