Consider one-dimensional conduction in a plane composite wall, as shown in Figure.The other outer surfaceof the wall has an emissivity of 0.8 and is exposed to quiescent air at 20 oC and radiation heat transfers.The temperature of the surroundings is 20 oC.
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