It will be implemented for flexibly moving and sensing inner problems.Small surface-mount device (SMD) components with motor drivers will be utilized to control the robot's motion.
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