Temperature Control and Data ProcessingThe temperature recorded in a thermogram is ideally the actual temperature be obtained by immersing a small thermocouple directly in the sample.Due to some possible catalytic decomposition of samples, potential contamination of samples, and mass measurement errors resulting from the thermocouple leads.Modern TGA systems use a computerized temperature control routine that automatically compares the voltage.
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