Additionally, the steady-state heat conduction equation is mentioned for modeling heat transmission through solid materials in a greenhouse, with a focus on heat transfer rates through frame and window materials.
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