A stochastic receding horizon approach to manage an EV chargingstation participating in DR programs for RECs has been proposed.Additional developments may regard the adaptation of the procedure todynamic traffic conditions, the integration of renewable resources, andthe experimental validation of the approach in real-world RECsThedeveloped procedure implements a stochastic approach that is (i) ableto exploit online information to schedule the EV charging such that theaggregated power consumption lies within prescribed energy boundsduring DR windows, and is (ii) computationally feasible to be deployedin real-world applications.Moreover, the computation timeremains feasible even for scenarios involving a high EV penetration.
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