Utilize MOSFETS to control the switching in the H-Bridge circuit, ensuring efficient motor direction changes.The DC motor operates on a 5V power supply, ensuring steady performance
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