Because the voltage across the windings depends on the iron losses as a result of that voltage during no load test approximately the rated voltage and the reason why we do not calculate copper loss because there is one current will flow magnetization current (no load)
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