3.Change the manual regulation ratio in software to 1.9V and start recording the time using the timer.V.3 71ENGINEERING TECHNOLOGY DEPARTMENTV.3 72a. Go to your computer, open Gunt software, and switch to the "RT 634 Pressure ControlDemonstration Unit" mode by clicking the arrows in the dialogue box as shown in Figure 6.4 (a). b. Click on "Charts" button as shown in Figure 6.4 (b).c. Set the "Software Controller" to "Manual" as shown in Figure 6.4 (c). d. In the "Manual Regulation Ratio" box, the maximum and minimum values that can be fed are 0Vto 10V which corresponds to the 0% to 100% opening of electrical proportional valve (9) as shownin Figure 6.4 (d).For this purpose, a step in control value is applied to the system in the non-regulated modeand the system's response observed.Fully close the extraction valve (8) by turning it clockwise and then open it less than 1/4th by turningthe knob 25 degrees in counter clockwise direction.Figure 6.4 Gunt Software Interface with steps7.Ask instructor to check.Procedure3.1.1.2.3.4.5.6.8.9.
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