Seatrest and BackrestSeatrest and Backrest are manufactured from polyurethane material in aluminum molds which are designed in accordance to the human anatomy and have the standart of 50 +- 10% densty and Mvss 302 fire behaviour.UpholsteryThe upholstery fabric is 100% polyester, has resistant to friction, non-flammable and have fastness properties.Foot and ArmrestThe legs are made of 18 mm mdf material and covered with laminated fabric The armrest is made of polished wooden from beech material.The Seatrest will have a gravity-centered mechanism that will allow it to close automatically.Seatrest and backrest are covered with whole specified properties fabric.
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