?Two halves of the mold must be tightly closed before the molten material is injectedinto the mold.The clamping of the mold is operated hydraulically, which it pushes the moving halfof the mold towards the fixed part to make an air tight chamber.???
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