Hysteresis in measuring instruments is caused by the lag between the input signal and the output reading of the instrument.This phenomenon occurs due to the mechanical or electrical properties of the materials used in the instrument, such as friction, magnetic properties, or elastic deformation.
تم تلخيص النص بواسطة موقع لخصلي © lakhasly.com
