The PID controller tuned with the root locus method clearly outperforms the Ziegler and Nichols tuning across most metrics, providing a better balance of precision, rapidity, and stability.The P controller, regardless of tuning method, generally performs poorly in comparison and requires significant improvements or a different control strategy.
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