1.Additionally, disturbance during sampling can change the soil structure and moisture content, leading to erroneous density measurements.If the dimensions of the cutter are not measured accurately or if there is a calibration issue with the weighing scale, the calculated density may be incorrect.2.
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