Switch on the power supply of the single top-pan balance and adjust its initial reading to zero by pressing the "TARE" button.
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