1.The empty filter is spun again to remove residual ethanol, and the silica filter is allowed to dry at room temperature.After filtration gel is added onto a silica spin column filter and centrifuged that will 2.Filtrate is discarded, and washing step repeated three times.2.3.4.