because of its good Si-SiO2 interface characteristics, whereas wet oxidation is used for thicker layers because of its higher growth rate After the oxidation process, a SiO2 layer is formed all over the wafer surface
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