Its made up of a number of stamping which are slotted to receive the windings.
 the stator carries a 3 phase winding and is fed from a 3 phase supply. 
it is wound for a definite number of poles p=2n ; where n is number a stator slots/pole/phase.
 
the exact number of poles being determined by the requirements of speed.
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