Such errors can be avoided by air-conditioning, magnetic shielding, cleaning the instruments, and housing the instruments properly depending on the application and type of the instrument
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