The diagram shown is a sketch of a relief valve.The pressure is applied directly on the spring seat as shown As the pressure applied, the force exerted on each bolt is 1000 N.The jomt stiffness constant is 36%.
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