1,850.0000 22.70 15% 643,522.50 SR2 Niagara Simplex Booster Pump, Horizontal End SuctionPump Model: FCm158 (01 Nos)Pump Flow rate = 1.07 LPS @ Head= 18 Mo Cast Iron Casing and SS304 Impellero Pump Inlet / Outlet Size = DN 25 / DN 25o Pressure Manager PS01AMotor Power= 1HP, 0.75KW- 3500rpm- 1x230V- 60H
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