Alternative lubricant additives must have friction-reducingphysicochemical properties and moderate costs comparedto those ofpetroleum oils before they can become widely accepted in themarketplace.Thecomparative analysis of several valuable friction-reducingphysicochemical properties indicated that the biodiesel obtained fromdistilled pyrolytic oil is a suitable lubricant additive for water-baseddrilling fluid.Lubricant additives are added to drilling fluids to lower thedrag and torque between the drill strings and rock formation.
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