As the rotor completes its rotation,the blades have to pass through aerodynamically dead zone which will result in lowering the system efficiency
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