Transpirational water flow in the xylem requires a mechanically strong wall that resists collapse in response to the negative pressure in the xylem.
Summarized by © lakhasly.com
