In onboard experiments, the LTE-Maritime router communicateswith onshore BSs while a ship sails along the plannedroute.In addition, for data transmission,a le transfer protocol (FTP) auto-call server was used whereDL, UL, and idle periods were set to 1, 1, and 3 minutes,respectively.