Buildings should be maintained in good repair and gutters and downpipes cleaned out atleast once a year.Roofs need to be checked annually to ensure that they are watertightand that roof coverings are securely fixed in place.
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