LPG is a viable alterna tive gaseous fuel (also known as ''Auto gas'') which is a gasproduct of petroleum refining primarily consisting of propane,propylene, butane and other light hydrocarbons [7-9].The engine, which uses conventional diesel fuel andLPG fuel, is referred to as 'LPG-Diesel dual fuel engine'.In contrast, the low cetane number of LPG makes it difficultto be used in large proportions in compression ignitionengines, mainly due to high cyclic variation [10,11,101].LPG has high calorificvalue compared to other gaseous fuels and also it has highoctane number but a low cetane number.The high octanenumber of LPG makes it suitable for spark ignition engines.Hence it can be used in the CI engine in the dual fuel modeonly and in this mode it has been extensively studied.So, storage and transportation ofLPG is easier than other gaseous fuels.It canbe liquefied in a low pressure range of 0.7-0.8 Mpa atatmospheric temperature.It leadsto better performance, low particulate and smoke emissions[12].
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