Explanation of the Code:analogRead(FSRPin): Reads the analog voltage from the FSR connected to pin A0.delay(500): Adds a half-second delay between readings to make the data more readable.
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