accessible buildings need 1500mm minimum (this width enables two trained people to carry a disabled person down in  the event of a fire).
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