The branch-line coupler is a four port network consisting of two main lines coupledby two quarter- wave length lines spaced by λ/4. Since the structure is reciprocal andsimmetrical the following conditions can be imposed on the scattering paramete
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