Weigh out the cement, sand, coarse aggregate and water separately as mentioned inthe concrete mix design.Place the weighted quantities of coarse aggregate, fine aggregate and the cement inthe pan or mixer.Fill the moulds (cube/cylinder) with obtained concrete in three layers of equal.height (approximately 50 mm).Each layer shall be uniformly tampered over the.the resulting concrete is of uniform color and proper workability.
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