In order to optimize the productivity of the Mishrif formation in the Al-Fakkah field, this investigation suggests the implementation of a Hydraulic Acid Fracturing treatment.The Mishrif formation's productivity has been substantially enhanced by this comprehensive approach.The maximum horizontal stress extends in a direction ranging from NE 20-80 degrees.To evaluate parameters such as fluid efficiency and fracture complexity, the MiniFrac treatment entailed injecting 150 barrels of #30 cross-linked gel at a rate of 25 barrels per minute, followed by an overflush with 30# linear gel.The paper meticulously documents all procedures before and after the treatment, emphasizing the importance of meticulous oversight to ensure safety, efficiency, and comprehensive documentation.Acid fracturing, a prevalent method for low-permeability limestone reservoirs, is advised.
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