When the steering wheel (helm) is turned, electrical power will travel to one of the solenoids and pull the valve ports into line sending hydraulic pressure down the system to a steering ram.
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