This happens because the current in the coil generatessufficient magnetic flux to attract the armature.Reset ismanual and rapid.
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