In this sieve analysis experiment, the particle size distribution of a solid substance was assessed by measuring the retained powder on a series of sieves with different-sized apertures.The specific percentage value of R200 (>50%) was used in determining the soil classification.The experiment was conducted with utmost precision, ensuring that the sieves were properly cleaned, the stack was securely fastened, and the weighing container captured all the sand particles.
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