METHOD:1.Switch on the air blower and place the vehicle (with the 5 five slotted masses on it) on the air track at the distance 0.5 m from the photogate.Prepare 5 slotted masses each with 10 g and put them evenly on the vehicle.Make a mass of the hanger using 5 g slotted mass and plasticine.Measure the mass of the system (The vehicle with 100 g and the 5 slotted masses and the mass hanger)5.Attach the thread to the vehicle at the end over the pulley to the hanger.3.4.6.7.8.
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