different users within the same physical LAN into different broadcast domains according to actual application requirements.
Summarized by © lakhasly.com
