In order to obtain anaerobic treatment of wastewater in more concentrated wastewater streams.The carbon gas produced consists mainly of 70% methane (CH4) and 30% carbon dioxide (CO2), with small amounts of other gases available.
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