Summarize this paragraph:Spray dryingThe drying of orange juice with each LAB culture and their control in RSM was carried out in a pilot-scale Spray Dryer (Niro Atomizer, Soborg, Denmark) with a vaned wheel rotating at high speed and a concurrent drying chamber (0.8 m diameter and 0.6 m height).Three replicates were conducted for each experiment.
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