A semi-permeable membrane is one that allows certain transfers of matter between two environments it separates while prohibiting others, or more generally, favoring some transfers over others. Reverse osmosis membranes are composed of a thin layer (active layer: skin) with a thickness between 0.1µm and 1.5µm, consisting of micropores.
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