When the supply power is first turned on, Vcap is 0 V, soVout will be HIGH• The capacitor will start charging toward the 5 V at Vout.• When Vcap reaches the positive-going threshold (VT+ ) ofthe Schmitt trigger, the output of the Schmitt will change to aLOW ( ~ 0V)• Now, with (Vout ~ 0) the capacitor will start dischargingtoward 0 V.• When Vcap drops below the negative-going threshold (VT- )the output of the Schmitt will change back to a HIGH.• The cycle repeats now, with the capacitor charging back up(VT+ ) to then down to (VT- ) then up to (VT+ ) and so on.• The waveform at Vout will be a square wave oscillatingbetween VOH and VOL, as shown
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