In the bus topology, the network .
all devices share single communication line or cable.
Bus topology may have problem while multiple hosts sending time.
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