Procedures:Grain length measured with calipers.12.Nitrogen cylinder connected to porosimeter; nitrogen passed through coil to reach it.3.Device had three valves, each serving a purpose; first valve maintained constant coil pressure (P1).9.Last valve opened to release nitrogen from porosimeter; nitrogen cylinder closed to prevent accidents.7.Two spacers inserted into cell; pressure read (coil pressure + cell pressure + spacer volume).
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