Geothermal energy is currently being harnessed through the extraction of hot fluids from two main sources: hydrothermal reservoirs with high permeability naturally, and Enhanced or engineered geothermal systems (EGS) with artificial fluid pathways.
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