The visual inspection was conducted with the test and control discs placed apart, not in direct contact with each other.Visual Accuracy Test To test visual accuracy in colour matching, the tests were conducted in a controlled environment at the Division of Prosthodontics and Implant Prosthodontics of the University of Genova, in complete darkness (
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