Loading and unloading of tire treads while rotating lead to the hysteresis loss and this loss is compensated by the engine of the vehicle, which effects the fuel efficiency.
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