Most configuration tasks can be done on the EtherChannel interface instead of on eachindividual port, ensuring configuration consistency throughout the links.When STP blocks one of the redundant links, it blocks the entireEtherChannel.When severalEtherChannel bundles exist between two switches, STP may block one of the bundles toprevent switching loops.o EtherChannel relies on existing switch ports.Where there is onlyone EtherChannel link, all physical links in the EtherChannel are active because STP sees onlyone (logical) link.
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